APIs in Category: vserver-peer-transition | Vserver API version 1.20

vserver-peer-transition-get vserver-peer-transition-get-iter | transition peer provides mechanism to setup relationships between a Data ONTAP 7-Mode system and a Data ONTAP Cluster-Mode Vserver. This relationship can be used by Cluster Admin to setup Snapmirror transition relationships or delegating these to Vserver Admin. These set of ZAPIs allow either to create or manage transition peer relationships.

NetApp Manage ONTAP

vserver-peer-transition-get | [top]

> Gets a transition peer relationship.

> Input Name | Range | Type | Description
> desired-attributes |  | vserver-peer-transition-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> local-vserver |  | vserver-name | Local Vserver name
> src-filer-name |  | string | Source 7-Mode system
> Output Name | Range | Type | Description
> attributes |  | vserver-peer-transition-info | The attributes of the vserver-peer-transition.

> Errno | Description
> EOBJECTNOTFOUND |  |
> EINTERNALERROR |  |

vserver-peer-transition-get-iter | [top]

> Gets list of transition peer relationship.

> Input Name | Range | Type | Description
> desired-attributes |  | vserver-peer-transition-info optional | Specify the attributes that should be returned. If not present, all attributes for which information is available will be returned. If present, only the desired attributes for which information is available will be returned.
> max-records | [1..2^32-1] | integer optional | The maximum number of records to return in this call. Default: 20
> query |  | vserver-peer-transition-info optional | A query that specifies which objects to return. A query could be specified on any number of attributes in the vserver-peer-transition object. All vserver-peer-transition objects matching this query up to 'max-records' will be returned.
> tag |  | string optional | Specify the tag from the last call. It is usually not specified for the first call. For subsequent calls, copy values from the 'next-tag' obtained from the previous call.
> Output Name | Range | Type | Description
> attributes-list |  | vserver-peer-transition-info[] optional | The list of attributes of vserver-peer-transition objects.
> next-tag |  | string optional | Tag for the next call. Not present when there are no more vserver-peer-transition objects to return.
> num-records | [0..2^32-1] | integer | The number of records returned in this call.

> Errno | Description
> EINTERNALERROR |  |

Element definition: vserver-name | [top]

> The name of the Vserver.

> [none]

Element definition: vserver-peer-transition-info | [top]

> Information about the transition peer. When returned as part of the output, all elements of this typedef are reported, unless limited by a set of desired attributes specified by the caller. When used as input to specify desired attributes to return, omitting a given element indicates that it shall not be returned in the output. In contrast, by providing an element (even with no value) the caller ensures that a value for that element will be returned, given that the value can be retrieved. When used as input to specify queries, any element can be omitted in which case the resulting set of objects is not constrained by any specific value of that attribute.

> Name | Range | Type | Description
> local-vserver |  | vserver-name optional | Local Vserver name Attributes: key, required-for-create, non-modifiable
> multi-path-address |  | string optional | Additional address for source 7-Mode system Attributes: optional-for-create, modifiable
> src-filer-name |  | string optional | Source 7-Mode system Attributes: key, required-for-create, non-modifiable

Element definition: vserver-name | [top]

> The name of the Vserver.

> [none]